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	Completed test form to be left in Maintenance Log  

Send a copy to the agency responsible for the annual inspection only if these tests are overdue

Do not send to DSPS for review unless requested
	


Hydraulic In-Ground Jack and/or Piping Test Report[image: image1.png]


 - Category 1
This applies to all in-ground jacks and piping regardless of installation contract date
This is not required for elevators where the jack(s) and all piping are above ground
Please type or print clearly.  Illegible and incomplete forms will not be accepted.
Personal information you provide may be used for secondary purposes [Privacy Law s. 15.04(1)(m), stats.]
	Conveyance Information

	Building Name:      
	Elevator Number:      

	Building Address:      
	Reg. Object ID or eSLA Permit No.: 

	Type
	Passenger   FORMCHECKBOX 

	Freight   FORMCHECKBOX 

	 LULA   FORMCHECKBOX 
  
	Part V or Private Res type in Commercial bldg.   FORMCHECKBOX 

	Special Purpose (SPPE)   FORMCHECKBOX 

	Sidewalk    FORMCHECKBOX 

	Stage/ Orch.   FORMCHECKBOX 


	Rated load (lbs):       
	Rated speed (up, fpm):      
	Rated or operating speed (down, fpm):      
	Leveling speed (fpm):      

	Date of Test:      
	PTO Year:        Test results can be used to satisfy either an overdue or future PTO but not both.  See SPS 318.17086 (14)


See SPS 318.17086(9)(b), (c) and (d), the code in effect when the conveyance or hydraulic jack were installed
and ASME A17.2.
	Relief Pressure – A17.1, 8.6.5.14.1

	Full-load working pressure (FLWP):       psi     Note: This is pressure in up direction with car fully loaded - this is not empty car running pressure

	FLWP determined by: (check one - calculation is not acceptable)  Verifying previous setting or records:  FORMCHECKBOX 
    Confirming now with test weights:  FORMCHECKBOX 
     

	Relief pressure (RP) with plunger or piston on stop-ring:       psi       Note: If RP exceeds 150% of FLWP, test will be rejected   

	Was pressure adjustment sealed prior to start of test: Yes:  FORMCHECKBOX 
  No:  FORMCHECKBOX 
  
	If no, will valve be sealed: Yes:  FORMCHECKBOX 
   No:  FORMCHECKBOX 
     
	If No, why:     

	

	Static Test – A17.1, 8.6.5.14.2

	After applying relief pressure to system open the main electrical disconnect for minimum 15 minutes.  A change in car position after the time has elapsed that cannot be explained by visible oil leakage, valve leakage or cooling of oil indicates a leak in the below-ground portion of the cylinder or piping.  To determine whether valve leakage occurred, the tester must compare the volume of oil rise in the tank to the volume of oil displaced from the cylinder by the plunger or piston during the test.

	Length of time for test (15 minutes minimum):       minutes  

	Change in oil level in tank:        inches
	Change in car position:       inches

	Corresponding change in oil volume in tank:       cubic inches
	Corresponding change in oil volume in cylinder:      cubic inches

	Does the descent of the car over the time match the rise in oil level in the tank?   Yes  FORMCHECKBOX 
  No  FORMCHECKBOX 
    
If no, explain where oil is lost:      

	

	Result of Test:  Pass  FORMCHECKBOX 
   Fail  FORMCHECKBOX 


	If Fail, elevator must be removed from service immediately per SPS 318.17086(9)(d).

Leaking in-ground jack or piping is under regulation of DNR for soil contamination.  Hydraulic jack or piping may not be abandoned in the ground. Elevator may not be placed out of service indefinitely or converted to a material lift where the elevator has failed one or both of these tests.  

	

	Tester Information

	Contractor Name (or Owner if performed by a licensed employee)                                             
	Individual Name
	     

	Address
	     
	License Number
	     
	Expiration Date
	     

	City
	
	State
	  
	ZIP
	     
	Signature


See ASME A17.1, 8.6.1.4.1, 8.6.1.7.2 and SPS 318.17086(5) for additional information regarding on-site records and test tags.
Per SPS 318.17086(4) periodic tests may be witnessed an inspector of the department, agent municipality or by a person authorized by the department or agent municipality.
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