|  |  |  |
| --- | --- | --- |
| DIVISION OF INDUSTRY SERVICES141 NW BARSTOW ST FL 4THWAUKESHA WI 53188-3789Contact Through Relay http://dsps.wi.gov/programs/industry-serviceswww.wisconsin.gov  | **Completed test form to be left in Maintenance Log** **Send a copy to the agency responsible for the annual inspection if these tests are overdue****Do not send to DSPS for review unless requested** |  |

# Elevator, Dumbwaiter and Material Lift Test Report

# Elevator - Acceptance and Category 5

# Dumbwaiter & Type B Material Lift - Acceptance

# (For Safety Device & Governor tests see form SBD 2E-E)

Please type or print clearly. Illegible and incomplete forms will not be accepted.

Personal information you provide may be used for secondary purposes [Privacy Law s. 15.04(1)(m), stats.]

|  |
| --- |
| **Conveyance Information** |
| Building Name:       | Conveyance No.:       |
| Building Address:       | Reg. Object ID or eSLA Permit No.:       |
| Type | Passenger[ ]  | Freight[ ]  | Comm. Inclined [ ]  | LULA [ ]  | Part V or Private Res type in a Commercial bldg [ ]  | Special Purpose (SPPE) [ ]  | Sidewalk[ ]  | Stage/ Orch. [ ]  | Dumbwaiter[ ]  | Type B Mat'l Lft [ ]  |
| Drive Type  | Electric Traction | Hydraulic  | Rack & Pinion ***(1)*** [ ]  | Screw ***(1)*** [ ]  | Hand ***(1)***[ ]  |
| Overhead[ ]  | Machine room-less [ ]  | Basement[ ]  | Winding drum [ ]  | Direct In Ground [ ]   | Direct Hole –less [ ]  | Roped [ ]  | Chained [ ]   |
| Rated load (lbs):       | Rated speed (up, fpm):       | Rated or operating speed (down, fpm):       | Leveling speed (fpm):       |
|  | **PTO Year**:       Test results can be used to satisfy either an overdue or future PTO but not both. See SPS 318.17086 (14) |

1. **These tests are required to be performed most commonly for Traction (8.6.4.20) and Hydraulic Elevators (8.6.5.16) however may also be required for Rack & Pinion (8.6.6.1.1), Screw (8.6.6.2.1), Hand (8.6.6.3.1) and Special Application (8.6.7) Elevators, Dumbwaiters and Type B Material Lifts (8.6.10.1.1 and 8.8.10.2.1 - acceptance).**

Also refer to the code in effect when the conveyance or applicable components were installed, unique manufacturer's procedures as addressed in ASME A17.1, 8.6.1.2.1(f) and 8.6.1.2.2(b), and ASME A17.2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Component, device or system** | Pass Fail n/a | Date | **Component, device or system** | Pass Fail n/a | Date |
| Safety device, Car See form SBD 2E-E | Trac. Brake sys,traction, tract. limit -125% ***(2)*** | [ ]  [ ]  [ ]  |       |
| Safety device, Cwt See form SBD 2E-E | Trac. Ascending car overspeed | [ ]  [ ]  [ ]  |       |
| Governor, switch, seal See form SBD 2E-E | Trac. Unintended movement -125% | [ ]  [ ]  [ ]  |       |
| Trac. Oil buffers Car [ ]  Cwt [ ]  | [ ]  [ ]  [ ]  |       | Hyd. Roped coated ropes | [ ]  [ ]  [ ]  |       |
| Trac. Driving machine brakes – 125% ***(2)*** | [ ]  [ ]  [ ]  |       | Hyd. Roped wire rope fastenings | [ ]  [ ]  [ ]  |       |
| Trac. Em. term. stopping & speed limiting | [ ]  [ ]  [ ]  |       | Hyd. Plunger gripper | [ ]  [ ]  [ ]  |       |
| Trac. Power opening of doors | [ ]  [ ]  [ ]  |       | Hyd. Overspeed valves | [ ]  [ ]  [ ]  |       |
| Trac. Leveling zone and leveling speed | [ ]  [ ]  [ ]  |       | Hyd. Freight sustain, level w/max load | [ ]  [ ]  [ ]  |       |
| Trac. Inner landing zone | [ ]  [ ]  [ ]  |       | All. Emerg communications | [ ]  [ ]  [ ]  |       |
| Alternative test methods meeting A17.1, 8.6.11.10, approved by the department and addressed in SPS 318.17086 (5)(c) & (12) may be used. If alternative test methods are used, attach the results. |
| **Tester Information** |
| Contractor Name (or Owner if performed by a licensed employee)       | Individual Name |       |
| Address |       | License Number |       | Expiration Date |       |
| City |       | State |    | ZIP |       | Signature |

# A copy of this completed test form or a similar record of results of the applicable tests must be located on site in the Maintenance Log according to SPS 318.17086(2)(g) 1 or 2 as applicable.

# Elevator test records and other required documentation are not to be accessed via an elevator car top. See ASME A17.1, 8.6.1.4.1, 8.6.1.7.2 and SPS 318.17086(5) for additional information regarding on-site records and test tags.

## **Per SPS 318.17086(4) periodic tests may be witnessed by an inspector of the department or agent municipality or person authorized by the department or agent municipality.**